#K$ Cam_ChangeAngleShiftTheta

Syntax 

Cam_ChangeAngleShiftTheta (CONSTANT, CONSTANT, REAL)
Description
Change the tolerance on the Theta angle. If AngleShiftTheta is greater than Pi,  no rotation is executed around the X axis..
CONSTANT:  0: the modification is permanent
		   1:  the modification is available only for the current frame.		
CONSTANT:  -1: restore the initial value 
		  0: add the third parameter to the current value of the field put the third parameter in the field
 		   1: put the third parameter in the field
REAL : 

Example(s)
Cam_ChangeAngleShiftTheta(1,1, 2.0)