#K$ Cam_IsFlagForcedAxis

Syntax 

Cam_IsFlagForcedAxis (CONSTANT)
Description
	Test if camera reference axis is currently forced with the Cam_ForceRefAxis () procedure.

	CONSTANT :	-1 : Initial value (test a permanent forced axis)
			 1 : Current value (test a temporary forced axis)
Example(s)